PUMP DATA:
MANUFACTURER ** MODEL NUMBER ** VOLTS**
OPERATING CONDITIONS:

WETWELL DIAMETER **
IMPELLER NUMBER ** 3 PHASE 60 HERTZ

HP**

RPM**

**	GPM AT **	TDH	**	% EFFICIENCY
SIZED FOR MINIMUM PUMP CYCLE TIME OF 12 MINUTES AND A MAXIMUM OF 6 PUMP STARTS PER HOUR. WORKING DEPTH **	FT.	WORKING VOLUME **	GALS.

℄

MINIMUM CONSTRUCTION STANDARDS FOR ST. LUCIE WEST SERVICES DISTRICT
450 SW UTILITY DRIVE, PORT SAINT LUCIE, FL 34986 PHONE: (772) 340-0220

LIFT STATION WET WELL SECTION (NO VALVE VAULT)

DETAIL: SLWS-13A DATE: 03/2020 SCALE: N.T.S. SHEET: 1 OF 2