(The following Qualified Products List defines the standard products approved by the SLWSD, however, the SLWSD reserves the right to make additions, deletions or to specify specific product use in certain situations.)

TABLE OF CONTENTS

Potable Water Products	6
ACCESS BOX AND COVER	6
AIR VALVE PEDESTAL HOUSING	6
AUTOMATIC FLUSHING DEVICE	6
BACKFLOW PREVENTERS  (Reduced Pressure Backflow Assembly)	6
BRONZE DISC VALVE MARKER	6
CASING SPACERS - 12" Width min	6
COMBINATION AIR VALVE (WATER) ONE-INCH (1")	6
COMBINATION AIR VALVE (WATER) TWO-INCH (2")	6
BALL CORPORATION STOP	7
DOUBLE CHECK ASSEMBLY	7
DOUBLE CHECK DETECTOR ASSEMBLY	7
DUCTILE IRON PIPE	7
DUCTILE IRON FITTINGS	7
ELECTRONIC MARKER BALLS WITH TIE DOWN STRAPS	7
FIRE HYDRANTS (5 1/4" VALVE OPENING)	7
HIGH DENSITY POLYETHYLENE PRESSURE PIPE OVER 3” DIAMETER	8
KEY VALVE BRANCH ASSEMBLY	8
KEY ANGLE METER VALVES	8
LOCATE TRACER WIRE	8
LOCATE TRACER WIRE CONNECTORS	8
LUBRICANT- (ANTI-SEIZE)	8
MARKING TAPE	8
MECHANICAL JOINT RESTRAINTS	8
METER BOXES CONCRETE & PLASTIC	9
PAINT FOR HYDRANTS, ABOVE GROUND APPURTANENCES, AND PIPING	9
PAINT FOR ALL UTILTY LIDS AND COVERS FLUSH WITH GROUND	9
PIPE RESTRAINTS	9
PIPE SUPPORTS	9
PRESSURE TRANSDUCER	9
POLYETHYLENE TUBING PE 3408 ONE-INCH (1")	9
POLYETHYLENE TUBING PE 3408 (2") (DIPS/CTS)	10
POLY PIGS	10

PVC PIPE	10
REFLECTIVE PAVEMENT MARKERS	10
SERVICE SADDLES (Stainless Steel Straps-Epoxy Coated)	10
TAPPING SADDLES (Stainless Steel)	10
VALVE BOX ALIGNMENT DEVICE	10
VALVE BOXES (SCREW TYPE) - WITH LOCKING LID	10
VALVE – TRUE UNION BALL	11
VALVE - GATE AND ANGLE - 3/4" - 3 "	11
VALVE – BUTTERFLY - RESILIENT SEAT	11
VALVES - CHECK - (Spring Loaded) (Swing Check)	11
VALVES – GATE - RESILIENT SEAT AND RESILIENT SEAT TAPPING	11
VALVE/TEE COMBINATION – GATE VALVE	11
WIRE PORT	11
Wastewater Products	12
ACCESS BOX AND COVER	12
AIR VALVE PEDESTAL HOUSING	12
BRONZE DISC VALVE MARKER	12
CASING SPACERS - 12" Width min	12
COATING (Concrete Exterior) – MANHOLES, WET WELLS, VALVE VAULTS, ABOVEGROUND TANKS, BUILDINGS	12
COMBINATION AIR VALVE (WASTEWATER)	12
CORPORATION STOP	12
CORROSION BARRIER SYSTEM FOR MANHOLES – NEW	13
CORROSION BARRIER SYSTEM FOR MANHOLES – REHABILITATION	13
DUCTILE IRON PIPE	13
DUCTILE IRON FITTINGS	13
ELASTOMERIC GASKET/ RESILIENT CONNECTORS (manholes)	13
ELECTRONIC MARKER BALLS WITH TIE DOWN STRAPS	13
EXTERNAL JOINT SEALING SYSTEMS	13
RUBBER JOINT SEALANT (manholes & wetwells)	14
HIGH DENSITY POLYETHYLENE PRESSURE PIPE OVER 3” DIAMETER	14
LOCATE TRACER WIRE	14
LOCATE TRACER WIRE CONNECTORS	14
LUBRICANT – (ANTI-SEIZE)	14
MANHOLE COVERS	14
MANHOLE INSIDE DROP ASSEMBLY	14
MARKING TAPE	14
MECHANICAL JOINT RESTRAINTS	15
METERS (Sewer)	15
PAINT FOR ABOVE GROUND APPURTANENCES, AND PIPING	15
PAINT FOR ALL UTILTY LIDS AND COVERS FLUSH WITH GROUND	15

PIPE RESTRAINTS	15
PIPE SUPPORTS	15
PRESSURE TRANSDUCER	16
POLY PIGS	16
POLYETHYLENE TUBING PE 3408 (2") (DIPS/CTS) – Green	16
PVC PIPE	16
PVC SEWER FITTINGS	16
reflective PAVEMENT MARKERS	16
SERVICE SADDLES (Stainless Steel Straps-Epoxy Coated Saddle)	16
TAPPING SLEEVE (Stainless Steel)	16
VALVE BOX ALIGNMENT DEVICE	17
VALVE BOXES (SCREW TYPE) - WITH LOCKING LID	17
VALVES - CHECK - (Spring Loaded) (Swing Check)	17
VALVE – TRUE UNION BALL	17
VALVE - GATE AND ANGLE - 3/4" - 3 "	17
VALVES – GATE - RESILIENT SEAT AND RESILIENT SEAT TAPPING	17
VALVES – PLUG	17
WIRE PORT	17
Reclaimed Water Products	18
ACCESS BOX AND COVER	18
AIR VALVE PEDESTAL HOUSING – purple	18
BRONZE DISC VALVE MARKER	18
CASING SPACERS - 12" Width min	18
COMBINATION AIR VALVE (WASTEWATER)	18
DUCTILE IRON PIPE	18
DUCTILE IRON FITTINGS	19
ELECTRONIC MARKER BALLS WITH TIE DOWN STRAPS	19
HIGH DENSITY POLYETHYLENE PRESSURE PIPE OVER 3” dIAMETER	19
LOCATE TRACER WIRE	19
LOCATE TRACER WIRE CONNECTORS	19
LUBRICANT – (ANTI-SEIZE)	19
MARKING TAPE	19
MECHANICAL JOINT RESTRAINTS	20
PAINT FOR ABOVE GROUND APPURTANENCES, AND PIPING	20
PAINT FOR ALL UTILTY LIDS AND COVERS FLUSH WITH GROUND	20
PIPE RESTRAINTS	20
PIPE SUPPORTS	20
POLY PIGS	20
PVC PIPE	20
REFLECTIVE PAVEMENT MARKERS	21

RECLAIMED WATER METER STATIONS	21
RUBBER JOINT SEALANT (MANHOLES & WETWELLS)	21
VALVE BOX ALIGNMENT DEVICE	21
VALVE BOXES (SCREW TYPE) - WITH LOCKING LID	21
VALVES - CHECK - (Spring Loaded) (Swing Check)	22
VALVE - GATE AND ANGLE - 3/4" - 3 "	22
VALVES – GATE - RESILIENT SEAT AND RESILIENT SEAT TAPPING	22
VALVES – PLUG	22
WIRE PORT	22
EXTERNAL JOINT SEALING SYSTEMS	23
CLEAN-OUT FRAME AND COVER	23
INTERCEPTORS – HAIR	23
INTERCEPTOR – LINT	23
INTERCEPTORS – GREASE (EXTERIOR)	23
INTERCEPTORS – GREASE (INTERIOR)	23
INTERCEPTORS – oil/sand	23
JOINT SEALANT	24
GREASE INTERCEPTOR COVERS	24
PAINT FOR ALL UTILTY LIDS AND COVERS FLUSH WITH GROUND	24
PVC PIPE	24
PVC SEWER FITTINGS	24
Pump Station Products	25
ACCESS BOX AND COVER	25
BRONZE DISC VALVE MARKER	25
COATING (Manholes & lift stations exterior)	25
CONTROL CABINET FASTENERS	25
CORROSION BARRIER SYSTEM FOR LIFT STATIONS – NEW	25
CORROSION BARRIER SYSTEM FOR LIFT STATIONS – REHABILITATION	25
DUCTILE IRON PIPE	25
DUCTILE IRON FITTINGS	26
ELASTOMERIC GASKET/ RESILIENT CONNECTORS (manholes)	26
ELECTRONIC MARKER BALLS WITH TIE DOWN STRAPS	26
EXTERNAL JOINT SEALING SYSTEMS	26
FALL THROUGH PREVENTION SYSTEMS	26
FLOATS	26
GENERATOR RECEPTACLE (lift station)	27
JOINT SEALANT (manholes & wetwells)	27
LOCATE TRACERWIRE	27
LOCATE TRACER WIRE CONNECTORS	27
LUBRICANT – (ANTI-SEIZE)	27

MARKING TAPE	27
MECHANICAL JOINT RESTRAINTS	27
ODOR/GAS SCRUBBER (lift station)	27
PAINT FOR ABOVE GROUND APPURTANENCES, AND PIPING	28
PAINT FOR ALL UTILTY LIDS AND COVERS FLUSH WITH GROUND	28
PIPE RESTRAINTS	28
PIPE SUPPORTS	28
PRESSURE TRANSDUCER	28
PUMP STATIONS	28
CONTROL PANELS	29
CONTROL PANELS COMPONENTS FOR LIFT STATIONS	29
Submersible Pumps	29
Wet Wells	29
Valve Vaults	30
PVC PIPE	30
PVC SEWER FITTINGS	30
REFLECTIVE PAVEMENT MARKERS	30
SIGNS	30
VALVE BOX ALIGNMENT DEVICE	30
VALVE BOXES (SCREW TYPE) - WITH LOCKING LID	30
VALVE - GATE AND ANGLE - 3/4" - 3"	30
VALVES – GATE - RESILIENT SEAT AND RESILIENT SEAT TAPPING	31
VALVES – PLUG	31
VALVES - CHECK - (Spring Loaded) (Swing Check)	31
VOLTAGE TRANSFORMER (Double Coil only)	31
WET WELL LINERS FOR REHABILITATION (Lift Stations/Manholes)	31
WIRE PORT	31

 POTABLE WATER PRODUCTS
ACCESS BOX AND COVER
(With WATER identification on lid)
Sigma VB-2763 X	b . USF 7630
AIR VALVE PEDESTAL HOUSING
Channell SPH142006C1B5L08A27
AUTOMATIC FLUSHING DEVICE

Environmental Enhancement & Technologies USA, Inc. HG-1 Hydro Guard
Eclipse 9700 – 2” Red Hydrant Flusher

BACKFLOW PREVENTERS (REDUCED PRESSURE BACKFLOW ASSEMBLY)

a. Ames 4000BSS (¾” - 2”) 4000SS (2 ½” – 10”)
b.    Febco 825Y (¾” - 2”) 825YP (2 ½” - 10”)
Golden Eagle 919 (¾” - 2”)

d. Watts 909LF (¾” - 10”) 919LF (¾” - 2”)
e. Wilkins 975XL2 (¾” - 2")
f.	Wilkins 375 (2 ½” - 10”)

BRONZE DISC VALVE MARKER

a.    R/G Wrenches & Extensions	b. Wager Company of Florida – WAGCO Marker

CASING SPACERS - 12" WIDTH MIN.

APS - Advance Products Systems
Cascade

PSI - Pipeline Seal and Insulator

COMBINATION AIR VALVE (WATER) ONE-INCH (1")
(Pipe Size 6" thru 10")

Apco 143C
ARI D-040

G.A. Industries 945

COMBINATION AIR VALVE (WATER) TWO-INCH (2")
(Pipe Size 12" and above)

Apco   145C	c . ARI D-040-C
G.A. Industries 945

BALL CORPORATION STOP

a. Mueller G-25028N (3/4” - 2")
b.    Ford FB1100-4-G-NL (1”)	c . Ford FB1100-7-G-NL (2”)

DOUBLE CHECK ASSEMBLY

a. Ames 200B (3/4” – 2”)
b. Ames 2000ss (2 ½” – 10”)
c.	Conbraco 40-100 (2 ½” – 10”)
d. Febco 805YP (2 ½” – 10”)

e. Watts 709LF (2 ½” – 10”)
f.	Wilkins 350XL(2” – 10”)
g. Wilkins 350XL(3/4” – 2”)

DOUBLE CHECK DETECTOR ASSEMBLY

a.    Ames 3000SS (2 ½" - 10")
b.    Conbraco 40-600 (3" - 10")
Febco 806Y DCDA (3” – 10”)

Watts 709 DCDA (3" - 10")
e. Wilkins 350DA (2 ½" - 12")

DUCTILE IRON PIPE
(Water - Cement Lined) (All flanged gaskets shall be full faced 1/8-inch Toruseal)

American
Clow (McWane)
Griffin

Tyler (McWane)
Union Foundry (McWane)
U.S. Pipe

DUCTILE IRON FITTINGS
(Water - Cement Lined) (All flanged gaskets shall be full faced 1/8-inch Toruseal)

American
Clow (McWane)
Griffin
Sigma

Star
Tyler (McWane)
Union Foundry (McWane)
U.S. Pipe

ELECTRONIC MARKER BALLS WITH TIE DOWN STRAPS

3M - Water/Blue 1403 XR
3M - Wastewater/Green 1404 XR

3M – Re-Use/Purple 1428 XR

FIRE HYDRANTS (5 1/4" VALVE OPENING)

AVK Nostalgic 2780
Mueller Super Centurion A-423
Clow Medallion

American Darling B-84-B Beach Side Spec

 HIGH DENSITY POLYETHYLENE PRESSURE PIPE OVER 3” DIAMETER

Driscoplex (Performance Pipe)
J-M Pipe
Polypipe, Inc

Rehau United

KEY VALVE BRANCH ASSEMBLY

a.    Ford UV43-42W-NL  (1" x 3/4")

KEY ANGLE METER VALVES

a. Ford BA43-342W-NL (1” x ¾”)	BA43-444W (1”)	BFA43-777W (2”)	
b. Mueller H-14258 (1” x ¾”)	H-14258 (1”)	H-14286 (2”)	

LOCATE TRACER WIRE

(Open-Cut Installation)
Copperhead Ind. Reinforced Tracer Wire (#12 AWG) #1230HS Blue

(Directional Boring Installation)
Copperhead Ind. Reinforced Tracer Wire (#12 EHS) #1245EHS Blue

LOCATE TRACER WIRE CONNECTORS

a. Copperhead Ind. DRYCONN Direct Bury Lug #CH90120

LUBRICANT- (ANTI-SEIZE)

a. Oxlic Never Seize

MARKING TAPE

a. Harris Industries – Blue – or SLWSD approved equal

MECHANICAL JOINT RESTRAINTS

American Fast Gasket
EBAA - Mega Lug
Ford - Uni-Flange
Sigma – SLD Series (DIP), SLC Series (PVC), PVPF Series (PVC to Pressure Fittings), ZF Series (Zip Flange)

U.S. Field-Lock Gasket
Star – Stargrip Series 3000
Romac Industries

METER BOXES CONCRETE & PLASTIC

Carson Plastic Box	Single 1419	Double 1220
Carson Plastic Solid T Cover Lid	Single 1419-4	Double 1220-4
Brooks Concrete	Single 36H	Double Dual-H

PAINT FOR HYDRANTS, ABOVE GROUND APPURTANENCES, AND PIPING

Safety Red – (fire hydrant)
Safety Blue – (potable water)

Safety Yellow – (private hydrants, bollards)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

PAINT FOR ALL UTILTY LIDS AND COVERS FLUSH WITH GROUND

Safety Red – (fire hydrants)	c. Safety Blue – (potable water)
Safety Yellow – (private hydrants)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

PIPE RESTRAINTS

Star – PVC Pipe Series 1000	c. Romac Industries
EBAA – Series 1500 and 2800	d. Sigma - PVP Series (PVC Bell & Spigot Joint)

PIPE SUPPORTS

Stainless Steel Stanchion Saddle Support (316 SS) (over 2”)
Unistrut Corp., Unistrut Metal Framing (316 SS) with Vinyl End Caps (up to 2”)

* Submit design to SLWSD for approval

PRESSURE TRANSDUCER

Water Main – Ashcroft –K1-5-M02-42-P7 100 PSI, with 6’ cord
Rosemount Analytical

POLYETHYLENE TUBING PE 3408 ONE-INCH (1")

Driscoplex (Performance Pipe)	c. Rehau United
Polypipe, Inc

POLYETHYLENE TUBING PE 3408 (2") (DIPS/CTS)

Driscoplex (Performance Pipe)	c. Polypipe, Inc
Rehau United

POLY PIGS

a.    Pigs - Knapp Polly Pig	b. Pig Signal Device – Maloney Pipeline Products

PVC PIPE

North American Pipe	d. Diamond Plastic Corporation
Silver Liner Plastics Inc.	e. J-M
National American

REFLECTIVE PAVEMENT MARKERS

3M	PSA 295 Blue
Ray-O-Lite	AA ARC II Blue
Hy-Viz	Rough Duty Stimsonite Model 911AB Blue

SERVICE SADDLES (STAINLESS STEEL STRAPS-EPOXY COATED)

Ford	c. JCM
Romac	d. Smith Blair (Rockwell)

TAPPING SADDLES (STAINLESS STEEL)

Cascade CST-EX	d. Ford – FAST
JCM #432	e. Power Seal #3490
Romac SST/SST-DB	f. Smith/Blair (Rockwell) #663

VALVE BOX ALIGNMENT DEVICE

a.    Adaptor, Inc. – Valve Box Adaptor II	b. Adaptor, Inc. – Valve Box Adaptor II – 6” PVC

VALVE BOXES (SCREW TYPE) - WITH LOCKING LID
(Valve Box and locking lid must be same manufacturer)

Tyler	c. Sigma Thickwall – Type X
Star - Type HD

VALVE – TRUE UNION BALL

a. Ipex - VX Series with EPDM seals or approved equal

VALVE - GATE AND ANGLE - 3/4" - 3 "

American Valve	d. AVK
Kennedy (McWane)	e. Milwaukee
Nibco

VALVE – BUTTERFLY - RESILIENT SEAT

Clow (McWane)	d. Dezurik
M & H (McWane)	e. Mueller
Pratt

VALVES - CHECK - (SPRING LOADED) (SWING CHECK)

American Flow Control (2"-36")	d. AVK (3 - 12”)
Clow (McWane) (2"-24")	e. Kennedy (McWane) (2"-24")
Mueller (2 ½"-24")	f. Valmatic

VALVES – GATE - RESILIENT SEAT AND RESILIENT SEAT TAPPING

American Flow Control	d. AVK
Clow (McWane)	e. Kennedy (McWane)
M & H(McWane)	f. Mueller

VALVE/TEE COMBINATION – GATE VALVE

a. AVK

WIRE PORT

a. Copperhead Industries – SnakePit Roadway Box with blue top

(END OF POTABLE WATER PRODUSTS LIST)

 WASTEWATER PRODUCTS

ACCESS BOX AND COVER
(With SEWER identification on lid)

a.    Sigma VB-2763 X	b. USF 7630

AIR VALVE PEDESTAL HOUSING

a. Channell SPH142006C1B5L08A27

BRONZE DISC VALVE MARKER

a.    R/G Wrenches & Extensions.	b. Wager Company of Florida – WAGCO Marker

CASING SPACERS - 12" WIDTH MIN.

APS - Advance Products Systems	c. Cascade
PSI - Pipeline Seal and Insulator

COATING (CONCRETE EXTERIOR) – MANHOLES, WET WELLS, VALVE VAULTS, ABOVEGROUND TANKS, BUILDINGS

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

COMBINATION AIR VALVE (WASTEWATER)

(2” Regular Body)
Apco	445	c. ARI D-020
G.A. Industries 942	d. Valmatic 802A

(2” Short Body)
a. ARI D-025

CORPORATION STOP

a.    Ford F1101-4 (1") FB1700-7 (2”)	b. Mueller H-15028 (1") H-10046 (2")

CORROSION BARRIER SYSTEM FOR MANHOLES – NEW

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

CORROSION BARRIER SYSTEM FOR MANHOLES – REHABILITATION

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

DUCTILE IRON PIPE
(Sewer - Epoxy Lined) (All flanged gaskets shall be full faced 1/8-inch SBR Rubber)

American	d . Clow (McWane)
Griffin	e. Tyler (McWane)
Union Foundry (McWane)	f. U.S. Pipe

DUCTILE IRON FITTINGS
(Sewer - Epoxy Lined) (All flanged gaskets shall be full faced 1/8 inch SBR Rubber)

American	e . Clow (McWane)
Griffin	f. Sigma
Star	g. Tyler (McWane)
Union Foundry (McWane)	h. U.S. Pipe

ELASTOMERIC GASKET/ RESILIENT CONNECTORS (MANHOLES)
(Prefabricated Pipe Boot)

Press-Seal Gasket Corporation, CAST-A-SEAL® 603 Cast-In Flexible Boot Connector Cored Holes
Press-Seal Gasket Corporation, PSX: DIRECT DRIVE

ELECTRONIC MARKER BALLS WITH TIE DOWN STRAPS

a. 3M - Wastewater/Green 1404 XR

EXTERNAL JOINT SEALING SYSTEMS

a.    CanUSA Wrapid Seal	b. Cretex Wrap

RUBBER JOINT SEALANT (MANHOLES & WETWELLS)
(Butyl Rubber Preformed Flexible Joint Sealant)

Press-Seal Gasket Corporation, PRO-STICK
Henry Company, RU106-RUB’ R-NEK “LTM”

HIGH DENSITY POLYETHYLENE PRESSURE PIPE OVER 3” DIAMETER

Driscoplex (Performance Pipe)
J-M Pipe

Polypipe, Inc
Rehau United

LOCATE TRACER WIRE
(Open-Cut Installation)
Copperhead Ind. Reinforced Tracer Wire (#12 AWG) #1230HS Green

(Directional Boring Installation)
Copperhead Ind. Reinforced Tracer Wire (#12 EHS) #1245EHS Green

LOCATE TRACER WIRE CONNECTORS

Copperhead Ind. DRYCONN Direct Bury Lug #CH90120

LUBRICANT – (ANTI-SEIZE)

Oxlic Never Seize

MANHOLE COVERS

CertainTeed Pamrex Ductile Iron Ring and Cover
U.S. Foundry & Manufacturing Corporation – USF 170 Cast Iron Ring and Cover

MANHOLE INSIDE DROP ASSEMBLY
*Submit to SLWSD for approval

MARKING TAPE

a. Arthur Enterprises / Harris Industries – Green – or approved equal

MECHANICAL JOINT RESTRAINTS

American Fast Gasket	g. EBAA - Mega Lug
Ford - Uni-Flange	h. U.S. Field-Lock Gasket
Star – Stargrip Series 3000, 4000
Romac Industries
Sigma – SLD Series (DIP), SLC Series (PVC), PVPF Series (PVC to Pressure Fittings),
ZF Series (Zip Flange)

METERS (SEWER)

Magnetic Flow Meter – Siemens Energy & Automation
Kamstrup
McCrometer – Ultramag

PAINT FOR ABOVE GROUND APPURTANENCES, AND PIPING

Safety Green – SW4085 (wastewater)
Brown – (wastewater)
Safety Yellow – SW4084 (bollards)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

PAINT FOR ALL UTILTY LIDS AND COVERS FLUSH WITH GROUND

a. Safety Green – (wastewater)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

PIPE RESTRAINTS

Star – PVC Pipe Series 1000	c. EBAA – Series 1500 and 2800
Romac Industries	d. Sigma - PVP Series (PVC Bell & Spigot Joint)

PIPE SUPPORTS

a. Stainless Steel Stanchion Saddle Support (316 SS)

*Submit design to SLWSD for approval

PRESSURE TRANSDUCER

Force Main – Ashcroft - K1-5-M02-42-P7 100 PSI, with 6’ cord
Rosemount Analytical

POLY PIGS

a.    Pigs - Knapp Polly Pig	b. Pig Signal Device – Maloney Pipeline Products

POLYETHYLENE TUBING PE 3408 (2") (DIPS/CTS) – GREEN

Driscoplex (Performance Pipe)
Polypipe, Inc
Rehau United

PVC PIPE

North American Pipe	d. Diamond Plastic Corporation
Silver Liner Plastics Inc.	e. J-M
National American

PVC SEWER FITTINGS

Harco	c. Plastic Trends
Multi Fittings

REFLECTIVE PAVEMENT MARKERS

3M	PSA 297 Green
Ray-O-Lite	AA ARC II Green
Hy-Viz Rough Duty Stimsonite Model 911AG Green

SERVICE SADDLES (STAINLESS STEEL STRAPS-EPOXY COATED SADDLE)

Ford	c. Smith Blair (Rockwell)
Romac Industries

TAPPING SLEEVE (STAINLESS STEEL)

Cascade CST-EX	d. Ford – FAST
JCM #432	e. Smith/Blair (Rockwell) #663
Romac SST

VALVE BOX ALIGNMENT DEVICE

a.    Adaptor, Inc. – Valve Box Adaptor II	b. Adaptor, Inc. – Valve Box Adaptor II – 6” PVC

VALVE BOXES (SCREW TYPE) - WITH LOCKING LID
(Valve Box and locking lid must be same manufacturer)

Tyler	c . Sigma Thickwall – Type X
Star - Type HD

VALVES - CHECK - (SPRING LOADED) (SWING CHECK)

American Flow Control (2"-36")	d. AVK (3 - 12”)
Clow (McWane) (2"-24")	e. Kennedy (McWane) (2"-24")
Mueller (2 ½"-24")	f. Valmatic

VALVE – TRUE UNION BALL

a. Ipex - VX Series with EPDM seals or approved equal

VALVE - GATE AND ANGLE - 3/4" - 3 "

American Valve
Kennedy (McWane)
Nibco

VALVES – GATE - RESILIENT SEAT AND RESILIENT SEAT TAPPING

American Flow Control	c. Kennedy (McWane)
Clow (McWane)	d. Mueller

VALVES – PLUG

Clow (McWane)	c.  Dezurik
Kennedy (McWane)	d. Milliken

WIRE PORT

a. Copperhead Industries – SnakePit Roadway Box with green top

(END OF WASTEWATER PRODUCTS LIST)

 RECLAIMED WATER PRODUCTS

ACCESS BOX AND COVER
(With Reclaimed Water or Reuse identification on lid)

a.    Sigma VB-2763 X	b. USF 7630

AIR VALVE PEDESTAL HOUSING – PURPLE

a. Channell SPH142006C1B5L08A27

BRONZE DISC VALVE MARKER

a.    R/G Wrenches & Extensions.	b. Wager Company of Florida – WAGCO Marker

CASING SPACERS - 12" WIDTH MIN.

APS - Advance Products Systems
Cascade
PSI - Pipeline Seal and Insulator

COMBINATION AIR VALVE (WASTEWATER)

(2” Regular Body)
Apco 445	c. G.A. Industries 942
Valmatic 802A	d. ARI D-020

(2” Short Body)
a.	ARI D-025

DUCTILE IRON PIPE
(Water - Cement Lined) (All flanged gaskets shall be full faced 1/8-inch SBR Rubber)

American	e. Clow (McWane)
Sigma	f . Star
Tyler (McWane)	g. U.S. Pipe
Union Foundry (McWane)

DUCTILE IRON FITTINGS
(Water - Cement Lined) (All flanged gaskets shall be full faced 1/8-inch SBR Rubber)

American	e. Clow (McWane)
Sigma	f . Star
Tyler (McWane)	g. U.S. Pipe
Union Foundry (McWane)

ELECTRONIC MARKER BALLS WITH TIE DOWN STRAPS

a. 3M – Re-Use/Purple 1428 XR

 HIGH DENSITY POLYETHYLENE PRESSURE PIPE OVER 3” DIAMETER

Driscoplex (Performance Pipe)	c. J-M Pipe
Polypipe, Inc	d. Rehau United

LOCATE TRACER WIRE

(Open-Cut Installation)
Copperhead Ind. Reinforced Tracer Wire (#12 AWG) #1230HS Purple

(Directional Boring Installation)
Copperhead Ind. Reinforced Tracer Wire (#12 EHS) #1245EHS Purple

LOCATE TRACER WIRE CONNECTORS

Copperhead Ind. DRYCONN Direct Bury Lug #CH90120

LUBRICANT – (ANTI-SEIZE)

a. Oxlic Never Seize

MARKING TAPE

a. Harris Industries – Purple

MECHANICAL JOINT RESTRAINTS

American Fast Gasket	f. EBAA - Mega Lug
Ford - Uni-Flange	g. U.S. Field-Lock Gasket
Star – Stargrip Series 3000, 4000
Romac Industries
Sigma – SLD Series (DIP), SLC Series (PVC), PVPF Series (PVC to Pressure Fittings), ZF Series(Zip Flange)

PAINT FOR ABOVE GROUND APPURTANENCES, AND PIPING

a. Purple – (REUSE)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

PAINT FOR ALL UTILTY LIDS AND COVERS FLUSH WITH GROUND

a. Purple – (REUSE)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

PIPE RESTRAINTS

Star – PVC Pipe Series 1000	c. Romac Industries
EBAA – Series 1500 and 2800	d. Sigma - PVP Series (PVC Bell & Spigot Joint)

PIPE SUPPORTS

Stainless Steel Stanchion Saddle Support (316 SS)
*Submit to SLWSD for approval

POLY PIGS

a.    Pigs - Knapp Polly Pig	b. Pig Signal Device – Maloney Pipeline Products

PVC PIPE

North American Pipe	c. Diamond Plastic Corporation
Silver Liner Plastics Inc.	d. J-M National American

REFLECTIVE PAVEMENT MARKERS

a. Hy-Viz Standard Duty Stimsonite Model 88AW Purple

RECLAIMED WATER METER STATIONS
Instrumentation/Systems Integrator – Integration Services Inc. (ISI)
Flow Meters –Kamstrup, McCrometer, Siemens with SS Trim & Gears, Flow Transmitter to have
4-20 mA analog output TR16 transmitter
Pressure Transmitters – Rosemount, with 1-100 psi range
Electric/Hydraulic Control Valve – Clay Val Specs to be submitted to SLWSD for approval.
Software – Ignition by Inductive
Enclosure – Stainless steel - to be submitted to SLWSD for approval.
Corrosion Inhibitor – to be submitted to SLWSD for approval.
Breakers – Square D
Pilot Lights, Selector Switches, Pushbuttons – Square D Type K
Terminal Blocks – Entrlec, Panduit, Square D
Surge Protection – Edco, Ditek, Square D
PLC – Allen Bradley, Delta, Modicon, Square D or approved equal
Control Relays – AA Electric, Square D, Diversified
DC/DC Converter – to be submitted to SLWSD for approval.
Batteries – Power Sonics, Yuasa, Werker (12V, 7.5 AH), APC or approved equal
Fiber Optic/Ethernet Swith – Cisco IE3000-4TC or approved equal
Optic Patch Panel – Corning, Anixter or approved equal
Fiber Optic/Modbus Converter – Lantronix XSDRSN-01 SPRESS-DR or approved equal
Level Transmitter – HydroRanger 200, Echomax XPS-5 Transducer
Digital Panel Display – Red Lion, Precision Digital, Allen Bradley, Square D

RUBBER JOINT SEALANT (MANHOLES & WETWELLS)
(Butyl Rubber Preformed Flexible Joint Sealant)

Press-Seal Gasket Corporation, PRO-STICK
Henry Company, RU106-RUB’ R-NEK “LTM”

VALVE BOX ALIGNMENT DEVICE

a.    Adaptor, Inc. – Valve Box Adaptor II	b. Adaptor, Inc. – Valve Box Adaptor II – 6” PVC

VALVE BOXES (SCREW TYPE) - WITH LOCKING LID
(Valve Box and locking lid must be same manufacturer)

Tyler	c. Sigma Thickwall – Type X
Star - Type HD

VALVES - CHECK - (SPRING LOADED) (SWING CHECK)

American Flow Control (2"-36")	d. AVK	(3 - 12”)
Clow (McWane) (2"-24")	e. Kennedy (McWane) (2"-24")
Mueller (2 ½"-24")	f. Valmatic

VALVE - GATE AND ANGLE - 3/4" - 3 "

American Valve
Kennedy (McWane)
Nibco

VALVES – GATE - RESILIENT SEAT AND RESILIENT SEAT TAPPING

American Flow Control	d. Mueller
Clow (McWane)
Kennedy (McWane)

VALVES – PLUG

Clow (McWane)	d. Dezurik
Homestead	e. Kennedy (McWane)
Milliken

WIRE PORT

Copperhead Industries – SnakePit Roadway Box with purple top

(END OF RECLAIMED WATER PRODUCTS LIST)

INTERCEPTOR PRODUCTS
*ALL INTERCEPTORS ARE TO BE SUBMITTED TO SLWSD FOR APPROVAL PRIOR TO INSTALLATION.

EXTERNAL JOINT SEALING SYSTEMS

a.    CanUSA Wrapid Seal	b. Cretex Wrap

CLEAN-OUT FRAME AND COVER

a.   Sigma VB-761	b. U.S. Foundry - USF 7630

INTERCEPTORS – HAIR

a.   Zurn	Z1175  or	Z1176

INTERCEPTOR – LINT

a. Zurn Z1185

INTERCEPTORS – GREASE (EXTERIOR)

a. Florida Septic Inc.	750 Grease	1050 Grease	1250 Grease	
b. Sebring Septic Tank	750 Grease	1050 Grease	1250 Grease	
American Concrete	750 SLW Grease	1050 SLW Grease 1250 SLW Grease
US Concrete	750 Grease	1050 Grease	1250 Grease
GREENTURTLE – Submit to SLWSD for approval.

INTERCEPTORS – GREASE (INTERIOR)

Thermaco	e. Big Dipper Internal Strainer (IS)
Highland Tank	f. G rease Stopper Automatic Grease Interceptors
GREENTURTLE- Submit to SLWSD for approval.

INTERCEPTORS – OIL/SAND

a. Florida Septic Inc.	750 Grease	1050 Grease	1250 Grease	
b. Sebring Septic Tank	750 Grease	1050 Grease	1250 Grease	
American Concrete	750 SLW Grease	1050 SLW Grease 1250 SLW Grease
US Concrete	750 Grease	1050 Grease	1250 Grease
GREENTURTLE – Submit to SLWSD for approval.

JOINT SEALANT
(Butyl Rubber Preformed Flexible Joint Sealant)

Press-Seal Gasket Corporation, PRO-STICK
Henry Company, RU106-RUB’ R-NEK “LTM”

GREASE INTERCEPTOR COVERS

CertainTeed Pamrex Ductile Iron Ring Cover
U.S. Foundry & Manufacturing Corporation – USF 170E Cast Iron Ring and Cover

PAINT FOR ALL UTILTY LIDS AND COVERS FLUSH WITH GROUND

a. Safety Green or Brown – (wastewater)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

PVC PIPE

North American Pipe	d. J-M
Diamond Plastic Corporation	e. National American
Silver liner Plastics Inc.

PVC SEWER FITTINGS

Harco
Multi Fittings
Plastic Trends

(END OF INTERCEPTOR PRODUCTS LIST)

 PUMP STATION PRODUCTS

ACCESS BOX AND COVER
(With appropriate WATER or SEWER identification on lid)

a.    Sigma VB-2763 X	b. USF 7630

BRONZE DISC VALVE MARKER

a.    R/G Wrenches & Extensions	b. Wager Company of Florida – WAGCO Marker

COATING (MANHOLES & LIFT STATIONS EXTERIOR)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

CONTROL CABINET FASTENERS
(Stainless Steel)
*Submit to SLWSD for approval

CORROSION BARRIER SYSTEM FOR LIFT STATIONS – NEW

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

CORROSION BARRIER SYSTEM FOR LIFT STATIONS – REHABILITATION

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

DUCTILE IRON PIPE
(Water - Cement Lined) (Sewer - Epoxy Lined) (All flanged gaskets shall be full faced 1/8-inch SBR Rubber)

American	d.   Clow (McWane)
Griffin	e.   Tyler (McWane)
Union Foundry (McWane)	f.	U.S. Pipe

DUCTILE IRON FITTINGS
(Water - Cement Lined) (Sewer - Epoxy Lined) (All flanged gaskets shall be full faced 1/8-inch SBR Rubber)

American	e. Clow (McWane)
Griffin	f. Sigma
Star	g. Tyler (McWane)
Union Foundry (McWane)	h. U.S. Pipe

ELASTOMERIC GASKET/ RESILIENT CONNECTORS (MANHOLES)
(Prefabricated Pipe Boot)

Press-Seal Gasket Corporation, CAST-A-SEAL® 603 Cast-In Flexible Boot Connector Cored Holes
Press-Seal Gasket Corporation, PSX: DIRECT DRIVE

ELECTRONIC MARKER BALLS WITH TIE DOWN STRAPS

a. 3M - Wastewater/Green 1404 XR

EXTERNAL JOINT SEALING SYSTEMS

CanUSA Wrapid Seal	b. Cretex Wrap

FALL THROUGH PREVENTION SYSTEMS
(Hatch Safety Grate)
U.S.F. Fabrication, Inc. (6’ diameter or larger wet wells)
Barneys Pump & Controls
*Submit to SLWSD for approval

(Hatch Safety Net)
U.S.F. Fabrication, Inc. (less than 6’ diameter wet wells)
Barneys Pump & Controls
*Submit to SLWSD for approval

FLOATS

Flygt-ENM-10
Myers
Roto Floats

GENERATOR RECEPTACLE (LIFT STATION)

a. Pyle-National JRE-4100 (up to 100 amps) or approved equal

JOINT SEALANT (MANHOLES & WETWELLS)
(Butyl Rubber Preformed Flexible Joint Sealant)

Press-Seal Gasket Corporation, PRO-STICK
Henry Company, RU106-RUB’ R-NEK “LTM”

LOCATE TRACERWIRE
(Open-Cut Installation)
Copperhead Ind. Reinforced Tracer Wire (#12 AWG) #1230HS Green

(Directional Boring Installation)
Copperhead Ind. Reinforced Tracer Wire (#12 EHS) #1245EHS Green

LOCATE TRACER WIRE CONNECTORS

a. Copperhead Ind. DRYCONN Direct Bury Lug #CH90120

LUBRICANT – (ANTI-SEIZE)

a. Oxlic Never Seize

MARKING TAPE

a. Harris Industries – Green

MECHANICAL JOINT RESTRAINTS

American Fast Gasket	f. EBAA - Mega Lug
Ford - Uni-Flange	g. U.S. Field-Lock Gasket
Star – Stargrip Series 3000, 4000
Romac Industries
Sigma – SLD Series (DIP), SLC Series (PVC), PVPF Series (PVC to Pressure Fittings), ZF Series(Zip Flange)

ODOR/GAS SCRUBBER (LIFT STATION)

a. Atlantic Environmental Systems, Inc. (MOPS) OGS-B-4,OGS-B-1036-4 Stage

PAINT FOR ABOVE GROUND APPURTANENCES, AND PIPING

Safety Green – (wastewater)
Safety Blue- (Potable Pump Stations)
Brown – (raw sewage above ground piping inside lift station fence)
Purple – (Reuse Pump Stations)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

PAINT FOR ALL UTILTY LIDS AND COVERS FLUSH WITH GROUND

Safety Green – (wastewater)
Safety Blue- (Potable Pump Stations)
Brown – (raw sewage above ground piping inside lift station fence)
Purple – (Reuse Pump Stations)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

PIPE RESTRAINTS

Star – PVC Pipe Series 1000	c. Romac Industries
EBAA – Series 1500 and 2800	d. Sigma - PVP Series (PVC Bell & Spigot Joint)

PIPE SUPPORTS

a. Stainless Steel Stanchion Saddle Support (316 SS)
*Submit to SLWSD for approval

PRESSURE TRANSDUCER

Force Main – Ashcroft, Rosemount
Water Service – Ashcroft, Rosemount
Reuse Irrigation Service- Ashcroft, Rosemount

PUMP STATIONS
(Private Grinders)
Myers (Hydro Pumps)
Atlantic Environmental Systems, Inc. (MOPS)

*Submit to SLWSD for approval

CONTROL PANELS

ECS Control Systems	c. Barneys Pumps
Best Controls Company	d. Integrated Services Inc (IS)

*Submit to SLWSD for approval

CONTROL PANELS COMPONENTS FOR LIFT STATIONS:
Surge Protection – Edco (analog) Polyphasor (radio), Square D (Electrical)
Corrosion Inhibitor – to be submitted to SLWSD for approval
Heliax Coaxial Cable and Connectors – to be submitted to SLWSD for approval
Terminal Blocks – Entrelec, Square D, Panduit
Control/Timing Relays – Square D, AA Electric, Diversified, Syrelec
DC/DC Converter – to be submitted to SLWSD for approval
Battery Charger – Xenotronics or approved equal
Batteries – Werker, Polysonics, Uuasa (12V, 7.5 AH minimum) or approved equal
Control Transformers – Square D
Motor Starters/VFD – Square D
Breakers – Square D
PLC – Allen-Bradley, Delta, Modicon, Square D or approved equal
Fiber/Ethernet Switch – Cisco
Fiber Patch Panel – to be submitted to SLWSD for approval
Fuses – Bussman, FuseLite
Phase Monitors/Alternators – Diversified
Unistrut Corp., Unistrut Metal Framing (316 SS) with Vinyl End Caps

SUBMERSIBLE PUMPS
(Private Grinders)
Myers (Hydro Pumps)
Homa (MOPS)

(SLWSD Owned Pumps Must be Non-Clog)

Flygt	d. Hydromatic
Homa	e. KSB
Barnes	f. ABB

WET WELLS
(Private Grinders)
Fiberglass
Myers (Hydro Pumps)
Atlantic Environmental Systems, Inc. (MOPS)

(SLWSD Owned)
Precast Concrete

American Concrete
US Concrete

VALVE VAULTS
(Private Grinders)
Fiberglass
Myers (Hydro Pumps)
Atlantic Environmental Systems, Inc. (MOPS)

(SLWSD Owned)
Precast Concrete
American Concrete
US Concrete

PVC PIPE

North American Pipe	d.	Diamond Plastic Corporation
Silver Liner Plastics Inc.	e.	J-M
National American

PVC SEWER FITTINGS

Harco
Multi Fittings
Plastic Trends

REFLECTIVE PAVEMENT MARKERS

3M	PSA 297 Green
Ray-O-Lite	AA ARC II Green
Hy-Viz	Rough Duty Stimsonite Model 911AG Green

SIGNS
*Submit to SLWSD for approval

VALVE BOX ALIGNMENT DEVICE

a.    Adaptor, Inc. – Valve Box Adaptor II	b. Adaptor, Inc. – Valve Box Adaptor II – 6” PVC

VALVE BOXES (SCREW TYPE) - WITH LOCKING LID
(Valve Box and locking lid must be same manufacturer)

a.   Tyler	b.	Star - Type HD

VALVE - GATE AND ANGLE - 3/4" - 3"

American Valve
Kennedy (McWane)
Nibco

VALVES – GATE - RESILIENT SEAT AND RESILIENT SEAT TAPPING

American Flow Control
Clow (McWane)	d. Kennedy (McWane)
M & H (McWane)	e. Mueller

VALVES – PLUG

Clow (McWane)	c. Dezurik
Kennedy (McWane)

VALVES - CHECK - (SPRING LOADED) (SWING CHECK)

American Flow Control (2"-36")	d. AVK (3 - 12”)
Clow (McWane) (2"-24")	e. Kennedy (McWane) (2"-24")
Mueller (2 ½"-24")	f. Valmatic

VOLTAGE TRANSFORMER (DOUBLE COIL ONLY)

General Electric	b. Square D

WET WELL LINERS FOR REHABILITATION (LIFT STATIONS/MANHOLES)

SLWSD owned – TNEMEC coating system required
*Private owned - Submit coating system to SLWSD for approval

WIRE PORT

Copperhead Industries – SnakePit Roadway Box with green top

(END OF PUMP STATION PRODUCTS LIST)